OE-MH GEN 1 A&E SPECIFICATIONS  
OPENEYE NVR CLOUD-MANAGED SERVER  
[www.openeye.net](http://www.openeye.net)

**DIVISION 28 – ELECTRONIC SAFETY AND SECURITY**

**28 20 00 Electronic Surveillance**

**28 23 00 Video Surveillance**

28 23 13 Video Surveillance Control and Management Systems

28 23 16 Video Surveillance Monitoring and Supervisory Interfaces

28 23 19 Digital Video Recorders and Analog Recording Devices

28 23 23 Video Surveillance Systems Infrastructure

28 23 26 Video Surveillance Remote Positioning Equipment

28 23 29 Video Surveillance Remote Devices and Sensors

**PART 1 GENERAL**

* 1. SUMMARY

1. This section includes the minimum requirements for Cloud-Managed NVR as a Service platform comprised of, but not limited to, the following components:
   1. Network Video Recorder Hardware
   2. Network Video Management Software
   3. Online Web Services
2. References
   1. 28 23 00 Video Surveillance
   2. 28 23 13 Video Surveillance Control and Management Systems
   3. 28 23 19 Digital Video Recorders and Analog Recording Devices
   4. 28 23 23 Video Surveillance Systems Infrastructure
   5. 28 23 29 Video Surveillance Remote Devices and Sensors
   6. SUBMITTALS
3. Manufacturer’s data sheets in digital or printed form.
4. Manufacturer’s installation and operations manuals in digital or printed form.
   1. QUALIFICATIONS
5. Manufacturer
   1. Manufacturer shall have been in business for more than 10 years.
6. Installer
   1. All installation, configuration, setup and related work shall be performed by an authorized technician certified by the manufacturer.
   2. All installation shall be performed by a technician licensed to install and service video surveillance and security equipment as mandated by the authority having jurisdiction.
   3. WARRANTY & SUPPORT
7. The Network Video Recorder shall come with a minimum 3 year manufacturer’s warranty with the 1st year including advance replacement service.
8. The Network Video Recorder shall come with a heroic customer service support structure, including a 1-888 number for technical service, pre and post sales assistance, and full access to online technical support as well as online sales support.
9. Technical support shall be available for 24 hours per day 7 days per week to all integrators and dealers free of charge.
10. System updates and patches shall be available free of charge.

- END OF SECTION -

PART 2 PRODUCTS

* 1. DOCUMENT SUMMARY

1. This document specifies the minimum criteria for the design and performance of the OE-MK Cloud-Managed Server.
   1. STANDARDS
2. The Network Video Recorder meets or exceeds the following requirements of the following publications and organizations.
   1. Joint Photographic Experts Group (JPEG)
   2. Moving Picture Experts Group (MPEG) (H.264/MPEG-4 Part 10 AVC)
   3. National Television System Committee (NTSC)
   4. Phase Alternation by Line (PAL)
   5. SYSTEM DESCRIPTION
3. The Network Video Recorder shall offer the latest in digital recording technology, product reliability, security, ease of use, and customer support structure.
4. The Network Video Recorder shall be offered in configurations up to 128 channels with a system wide recording bitrate of up to 400Mbps.
   1. OPERATING SPECIFICATIONS
5. Environmental Conditions: the Network Video Recorder shall be designed to operate under the following environmental specifications:
   1. Operating Temperature: 40°F to 104°F (5°C to 40°C) non-condensing.
6. Power Requirements: Recorder shall have the following electrical specifications:

A. Power Requirement: 115 – 230 VAC

1. Max Power Consumption: 300W
2. Product Label Requirements:
   1. The Network Video Recorder shall have the FCC and ETL (Intertek) certifications clearly marked on the product and box label.
      1. Dimensions: W: 17.25 x H: 5.2 x D: 26in (438 x 132 x 660mm).
      2. Weight: 77lbs (34.9kg)
   2. OPERATIONAL REQUIREMENTS
3. NVR Cloud-Managed Server – The network video recorder shall include, as a minimum, the following features/functions/specifications. The network video recorder shall:
   * + 1. Be assembled in the U.S.A
       2. Include an Intel i7 processor.
       3. Include 16 Gigabytes of DDR4 system memory
       4. Include dual 10/100/1000 Network Interface connections.
       5. Provide one dedicated Intel GbE network port for Client Networks and one dedicated Intel GbE network port for Camera Networks.
       6. Be optimized for and support the Windows Embedded Operating System.
       7. Provide recording support for high resolution Megapixel HD IP video.
       8. Include remote capabilities including free VMS and mobile applications for Apple and Android devices.
       9. Include the ability to unlock additional IP camera licenses offering up to a combined total of 128 IP cameras per NVR with a maximum recording throughput of 400Mbps on RAID models and 300Mbps on JBOD models.
       10. Support static IP and DHCP IP addressing through user configurable TCP/IP settings.
       11. Be capable of recording up to 30 IPS on a single channel in an environment where all channels are being utilized.
       12. Come standard with a single Solid State Drive (SSD) on the NVR JBOD model exclusively dedicated to the Operating System. No Video will be allocated to the SSDs for the purposes of video storage or archiving.
       13. Come standard with dual Solid State Drives (SSD) configured in a RAID 1 array on the NVR RAID model exclusively dedicated to the Operating System. No Video will be allocated to the SSDs for the purposes of video storage or archiving.
       14. Offer the following on-board hard drive capacity options with up to sixteen internally installed, front removable hard drive bays:
           1. 24.0 Terabytes
           2. 30.0 Terabytes
           3. 36.0 Terabytes
           4. 48.0 Terabytes
           5. 64.0 Terabytes
           6. 96.0 Terabytes
           7. 128.0 Terabytes
           8. 160.0 Terabytes
           9. 192.0 Terabytes
       15. Provide a server grade cooling design that allows maximum internal cooling through five high output 80mm fans mounted in the center of the chassis.
       16. Include a separate dedicated RAID 5 controller Card configured exclusively for video recording on the NVR RAID models. All RAID 5 resource load shall be handled on the RAID 5 card exclusively and shall not utilize resources from the motherboard’s on-board processor. RAID management software will be included with every NVR RAID model.
       17. Only use high performance Video Surveillance rated hard drives engineered for reliability and 24x7 “always on” environments for the NVR JBOD models.
       18. Only use high performance Enterprise rated hard drives engineered for reliability and 24x7 “always on” “RAID” environments.
       19. Be housed in a rackmount 3U 16-Bay server chassis designed to fit into a 19” EIA rack.
       20. Allow for Plug and Play connection with OpenEye or ONVIF cameras.
       21. Provide a full auto-switching power supply rated at 650W
       22. Support up to 4K maximum display resolution
       23. Have the ability to easily backup important video to an external cloud-managed location, DVD-R media or a USB device. The recorder must not stop recording during the backup process. To ensure the integrity of data, the cloud-managed appliance shall use a proprietary viewer that can detect image tampering.
       24. Include a minimum of the following front panel controls:
           1. Two 2.0 USB ports
       25. Include a minimum of the following rear-panel connectors:
           1. One Power input
           2. Four USB 3.0 inputs
           3. Two USB 2.0 inputs
           4. Two HDMI connectors with a maximum 4K display resolution
           5. One DVI-D connector with a maximum 1080P display resolution
           6. One DVI-I connector with a maximum 1080P display resolution
           7. Two 10/100/1000 RJ-45 Network Ports
           8. Line in / Speaker out – RCA
       26. Include the following components:
           1. USB Mouse
           2. USB Keyboard QWERTY
           3. System Recovery USB
           4. Power Cord
           5. User Quick Start Guide
           6. Rack Mount Installation Kit
           7. Rack Mount Rail Kit
           8. OpenEye branded front locking bezel
4. LIST OF SUPPORTED MODELS
   1. The Network Video Recorder shall be one of the following models or an approved equivalent:

|  |  |
| --- | --- |
| OE-MHX24\* | Enterprise 3U Server w/ Windows OS, and 24TB |
| OE-MHX30\* | Enterprise 3U Server w/ Windows OS, and 30TB |
| OE-MHX36\* | Enterprise 3U Server w/ Windows OS, and 36TB |
| OE-MHX48\* | Enterprise 3U Server w/ Windows OS, and 48TB |
| OE-MHX64\* | Enterprise 3U Server w/ Windows OS, and 64TB |
| OE-MHX96\* | Enterprise 3U Server w/ Windows OS, and 96TB |
| OE-MHX128\* | Enterprise 3U Server w/ Windows OS, and 128TB |
| OE-MHX160\* | Enterprise 3U Server w/ Windows OS, and 160TB |
| OE-MHX192\* | Enterprise 3U Server w/ Windows OS, and 192TB |
| OE-MHX24R\* | Enterprise 3U Server w/ Windows OS, and 24TB RAID 5 (20TB Usable) |
| OE-MHX30R\* | Enterprise 3U Server w/ Windows OS, and 30TB RAID 5 (24TB Usable) |
| OE-MHX36R\* | Enterprise 3U Server w/ Windows OS, and 36TB RAID 5 (32TB Usable) |
| OE-MHX48R\* | Enterprise 3U Server w/ Windows OS, and 48TB RAID 5 (44TB Usable) |
| OE-MHX64R\* | Enterprise 3U Server w/ Windows OS, and 64TB RAID 5 (60TB Usable) |
| OE-MHX96R\* | Enterprise 3U Server w/ Windows OS, and 96TB RAID 5 (96TB Usable) |

\* (Appliance Software and OWS Licensing Sold Separately)

**PART 3 EXECUTION**

* 1. INSTALLATION

1. Installer shall comply with all instructions and best practices specified by the hardware and software manufacturer.
2. Installer shall comply with all applicable state and local regulatory requirements.
   1. STORAGE
3. Equipment shall be stored in environmental conditions within the stated temperature and humidity ranges specified by the hardware manufacturer.
   1. COMISSIONING
4. The manufacturer shall offer the option for factory pre-configuration of all hardware and software purchased from the manufacturer as an additional paid service.
5. The manufacturer shall offer the option for remote or in person system commissioning as an additional paid service.

- END OF SECTION -

END OF DOCUMENT